{
    "noclone": false,
    "mode": "FDM",
    "internal": 0,
    "bedHeight": 2.5,
    "bedWidth": 222,
    "bedDepth": 222,
    "bedRound": false,
    "bedBelt": false,
    "resolutionX": 1600,
    "resolutionY": 900,
    "maxHeight": 222,
    "originCenter": false,
    "extrudeAbs": false,
    "gcodeFan": [
        "M106 S{fan_speed}"
    ],
    "gcodeTrack": [
        "M117 {progress}% layer {layer} / {layers}"
    ],
    "gcodeLayer": [],
    "gcodePre": [
        "M107                         ; turn off filament cooling fan",
        "M104 S{temp} T0              ; set extruder temperature",
        "M140 S{bed_temp} T0          ; set bed temperature",
        "G90                          ; set absolute positioning mode",
        "M83                          ; set relative positioning for extruder",
        "G28                          ; home axes",
        "G1 F3000                     ; set default move speed",
        "G1 Z1 F6000                  ; pause above the bed",
        "M190 S{bed_temp} T0          ; wait for bed to reach target temp",
        "M109 S{temp} T0              ; wait for extruder to reach target temp",
        "G92 E0                       ; set extruder position to 0"
    ],
    "gcodePost": [
        "M107                ; turn off filament cooling fan",
        "M104 S0 T0          ; turn off extruder",
        "M140 S0 T0          ; turn off bed",
        "G91                 ; relative movement",
        "G1 Z10 F1200        ; drop bed 10mm",
        "G90                 ; absolute positioning",
        "G28 X0 Y0           ; home XY axes",
        "M84                 ; disable stepper motors"
    ],
    "gcodeExt": [],
    "gcodeInt": [],
    "gcodeProc": "",
    "gcodePause": [],
    "gcodeDwell": [],
    "gcodeSpindle": [],
    "gcodeChange": [],
    "gcodeFExt": "gcode",
    "gcodeSpace": true,
    "gcodeStrip": false,
    "gcodeLaserOn": [],
    "gcodeLaserOff": [],
    "extruders": [
        {
            "extFilament": 1.75,
            "extNozzle": 0.4,
            "extSelect": [
                "T0"
            ],
            "extDeselect": [],
            "extOffsetX": 0,
            "extOffsetY": 0
        }
    ],
    "deviceName": "Anycubic Kobra",
    "fwRetract": false,
    "extras": {
        "palette": {
            "printer": "6c99ea036da",
            "ping": null,
            "feed": null,
            "push": null,
            "offset": null,
            "heat": null,
            "cool": null,
            "press": null
        }
    }
}
